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a2A2600-64umBAS
The a2A2600-64umBAS Basler ace 2 R camera is equipped with a Gpixel GMAX2505 sensor.
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Specifications
General Specifications
	
	a2A2600-64umBAS

	Resolution (H x V Pixels)
	2600 x 2160 (full resolution)
2600 x 2128 (default resolution)

	Resolution
	5 MP

	Sensor Type
	GMAX2505
Progressive scan CMOS
Global shutter

	Sensor Format
	1/2"

	Effective Sensor Diagonal
	8.45 mm

	Pixel Size (H x V)
	2.5 x 2.5 µm

	Frame Rate (at Default Settings)
	65.0 fps
70.4 fps (Device Link Throughput Limit mode set to Off)

	Product Family
	ace 2 R

	Mono / Color
	Mono

	Image Data Interface
	USB 3.0, nominal max. 5 Gbit/s (SuperSpeed)

	Pixel Formats
	See Pixel Format.

	Synchronization
	Via hardware trigger
Via software trigger
Via free run

	Exposure Time Control
	Via hardware trigger
Programmable via the camera API

	Camera Power Requirements
	≈2.7 W (typical) @ 5 VDC

	I/O Lines
	1 opto-coupled input line
2 general purpose I/O (GPIO) lines

	Lens Mount
	C-mount

	Size (L x W x H)
	36.3 x 29 x 29 mm (without lens mount or connectors)
48.1 x 29 x 29 mm (with lens mount and connectors)

	Weight
	<85 g

	Conformity
	CE (includes RoHS), EAC, UL Listed, FCC, KC, GenICam, USB3 Vision, IP30
Certificates for your camera model
For more information, see the Compliance section of the Basler website.

	Software
	Basler pylon Software Suite (version 6.0 or higher)
Available for Windows, Linux x86, Linux ARM, macOS, and Android

	Accessories
	Lenses – 
C125-0418-5M-P f4mm	2000034830
C125-0618-5M-P f6mm	2000034831
C125-0818-5M-P f8mm	2000034832
C125-1218-5M-P f12mm	2000034833
C125-1620-5M-P f16mm	2000034834
C125-2522-5M-P f25mm 	2000034835




Cables – 
USB Cable - with screwlock	2200000620
USB Cable - with screwlock	2200000621
USB Cable - without screwlock	2000035131
USB Cable - without screwlock	2000035315
M8, 5m, axial - Lighting Cable	2200000899
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Dimensions in mm
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  Please contact OEM Automatic for technical   assistance.   Email:  vision@oem.co.uk   Telephone : 01162849900  


image4.png




image5.png
BASLER’




