**a2A4200-12gcBAS**

The a2A4200-12gcBAS Basler ace 2 R camera is equipped with a Gpixel GMAX2509 sensor.



**Specifications**

**General Specifications**

|  | a2A4200-12gcBAS |
| --- | --- |
| Resolution (H x V Pixels) | 4200 x 2160 (full resolution)4200 x 2128 (default resolution) |
| Resolution | 9 MP |
| Sensor Type | GMAX2509Progressive scan CMOSGlobal shutter |
| Sensor Format | 2/3" |
| Effective Sensor Diagonal | 11.81 mm |
| Pixel Size (H x V) | 2.5 x 2.5 µm |
| Frame Rate (at Default Settings) | 11.5 fps13.0 fps (with Bandwidth Reserve mode set to Performance and packet size set to 4000) |
| Product Family | ace 2 R |
| Mono / Color | Colour |
| Image Data Interface | Fast Ethernet (100 Mbit/s)Gigabit Ethernet (1000 Mbit/s) |
| Pixel Formats | See Pixel Format. |
| Synchronization | Via hardware triggerVia software triggerVia free run |
| Exposure Time Control | Via hardware triggerProgrammable via the camera API |
| Camera Power Requirements | ≈4.5 W (typical) when using Power over Ethernet≈3.4 W (typical) @ 12–24 VDC when supplied via I/O connector |
| I/O Lines | 1 opto-coupled input line2 general purpose I/O (GPIO) lines |
| Lens Mount | C-mount |
| Size (L x W x H) | 48.9 x 29 x 29 mm (without lens mount or connectors)62.2 x 29 x 29 mm (with lens mount and connectors) |
| Weight | <100 g |
| Conformity | CE (includes RoHS), EAC, UL Listed, FCC, KC, GenICam, GigE Vision, IP30, IEEE 802.3af (PoE)Certificates for your camera modelFor more information, see the Compliance section of the Basler website. |
| Software | Basler pylon Software Suite (version 6.0 or higher)Available for Windows, Linux x86, Linux ARM, macOS, and Android |
| Accessories | Lenses – C125-0418-5M-P f4mm 2000034830C125-0618-5M-P f6mm 2000034831C125-0818-5M-P f8mm 2000034832C125-1218-5M-P f12mm 2000034833C125-1620-5M-P f16mm 2000034834C125-2522-5M-P f25mm 2000034835 |

 Cables –

GigE Cable - with screwlock 2200000622

M8, 5m, axial - Lighting Cable 2200000899

Drawing –

Please contact OEM Automatic for technical assistance.

Email: vision@oem.co.uk

Telephone: 01162849900