**a2A4200-12gcBAS**

The a2A4200-12gcBAS Basler ace 2 R camera is equipped with a Gpixel GMAX2509 sensor.



**Specifications**

**General Specifications**

|  | a2A4200-12gcBAS |
| --- | --- |
| Resolution (H x V Pixels) | 4200 x 2160 (full resolution) 4200 x 2128 (default resolution) |
| Resolution | 9 MP |
| Sensor Type | GMAX2509 Progressive scan CMOS Global shutter |
| Sensor Format | 2/3" |
| Effective Sensor Diagonal | 11.81 mm |
| Pixel Size (H x V) | 2.5 x 2.5 µm |
| Frame Rate (at Default Settings) | 11.5 fps 13.0 fps (with Bandwidth Reserve mode set to Performance and packet size set to 4000) |
| Product Family | ace 2 R |
| Mono / Color | Colour |
| Image Data Interface | Fast Ethernet (100 Mbit/s) Gigabit Ethernet (1000 Mbit/s) |
| Pixel Formats | See Pixel Format. |
| Synchronization | Via hardware trigger Via software trigger Via free run |
| Exposure Time Control | Via hardware trigger Programmable via the camera API |
| Camera Power Requirements | ≈4.5 W (typical) when using Power over Ethernet ≈3.4 W (typical) @ 12–24 VDC when supplied via I/O connector |
| I/O Lines | 1 opto-coupled input line 2 general purpose I/O (GPIO) lines |
| Lens Mount | C-mount |
| Size (L x W x H) | 48.9 x 29 x 29 mm (without lens mount or connectors) 62.2 x 29 x 29 mm (with lens mount and connectors) |
| Weight | <100 g |
| Conformity | CE (includes RoHS), EAC, UL Listed, FCC, KC, GenICam, GigE Vision, IP30, IEEE 802.3af (PoE) Certificates for your camera model For more information, see the Compliance section of the Basler website. |
| Software | Basler pylon Software Suite (version 6.0 or higher) Available for Windows, Linux x86, Linux ARM, macOS, and Android |
| Accessories | Lenses –  C125-0418-5M-P f4mm 2000034830  C125-0618-5M-P f6mm 2000034831  C125-0818-5M-P f8mm 2000034832  C125-1218-5M-P f12mm 2000034833  C125-1620-5M-P f16mm 2000034834  C125-2522-5M-P f25mm 2000034835 |

Cables –

GigE Cable - with screwlock 2200000622

M8, 5m, axial - Lighting Cable 2200000899

A diagram of a machine

Description automatically generated with medium confidenceDrawing –

Please contact OEM Automatic for technical assistance.

Email: [vision@oem.co.uk](mailto:vision@oem.co.uk)

Telephone: 01162849900