**daA3840-45uc – S-Mount**

The daA3840-45uc Basler dart USB 3.0 camera module is equipped with a Sony IMX334 sensor.



**Variants**

**S-mount:** Consists of a circuit board and a camera front. S-mount lenses can be mounted in the lens mount on the camera front.

**Specifications**

**General Specifications**

|  | daA3840-45uc |
| --- | --- |
| Resolution (H x V Pixels) | 3860 x 2178 (full resolution)3840 x 2160 (default resolution) |
| Resolution | 8.3 MP |
| Sensor Type | Sony IMX334LLR-CProgressive scan CMOSRolling shutter |
| Sensor Format | 1/1.8" |
| Effective Sensor Diagonal | 8.86 mm |
| Pixel Size (H x V) | 2.0 x 2.0 µm |
| Frame Rate | 18.7 fps (default settings)44.9 fps (default settings, disabled Device Link Throughput Limit) |
| Mono / Color | Colour |
| Image Data Interface | USB 3.0, nominal max. 5 Gbit/s (SuperSpeed) |
| Pixel Formats | See Pixel Format. |
| Synchronization | Via hardware triggerVia software triggerVia free run |
| Exposure Time Control | Programmable via the camera API |
| Camera Power Requirements | ≈1.7 W (typical) @ 5 VDC |
| I/O Lines | 4 general purpose I/O (GPIO) lines |
| Lens Mount | S-mount, CS-mount, without mount (bare board) |
| Size (L x W x H) | S-mount and CS-mount models: 20 x 29 x 29 mmBare board model: 8 x 28.3 x 27 mm |
| Weight | S-mount and CS-mount models: <15 gBare board model: <5 g |
| Conformity | CE (includes RoHS), EAC, UL Listed, GenICam 2.x (including PFNC 1.x and SFNC 2.x), USB3 Vision, REACH, FCC, KCCertificates for your camera modelFor more information, see the Compliance section of the Basler website. |
| Software | Basler pylon Software Suite (version 6.0 or higher)Available for Windows, Linux x86, Linux ARM, macOS, and Android |
| Accessories | Lenses – Evetar Lens E3417A F2.4 f2.5mm 1/1.8" 2200001056Evetar E3417A IR-Cut F2.4 f2.5mm 1/1.8" 2200001057Evetar Lens E3360A F2.0 f4.0mm 1/1.8" 2200001058Evetar E3360D IR-Cut F2.0 f4mm 1/1.8” 2200000589Evetar Lens E3388 F2.6 f7.8mm 1/1.8" 2200001060Evetar E3388 IR-Cut F2.6 f7.8mm 1/1.8" 2200001061Cables - USB Cable - with screwlock 2200000620USB Cable - with screwlock 2200000621USB Cable - without screwlock 2000035131USB Cable - without screwlock 2000035315GigE Cable - with screwlock 2200000622Mounting Covers – Dart Mounting Cover 2200000959 |

Drawing –



